|  | ## SONIC1 Pair Setup

Sampling |
--- | ---
piezo_hz: |
chirp: |
txgain: |
rxgain: |
window: |
samp_hz: |
samp_sz: |
period: |
Time-of-Flight Detector | --
scale_out_min: |
scale_out_max: |
sensitivity: |
low_pass: |
zero_cut: |
segment_sz: |
discriminator: |
tolerance: |
duration: |
offset: |
correction: |
preset: |

Flow Chamber Geometry | --
--- | ---
opposite: |
adjacent: |
hypotenuse: |
area: |
sign: |
Ultrasonic Pair | --
sensor_id[0]: |
sensor_id[1]: |